these are the impulse responses recorded with the b+k dummy head.
dummy head height: 1630mm above floor level
floor is damped

recordings done by Martin Rumori 2008-04-03
http://lac.linuxaudio.org/2013/papers/60.pdf

ear channel/headphone correction (HD600) and stereo file merging applied by Matthias Kronlachner, April 2013


h1: ear channel 1370mm above floor level

h2: ear channel 1630mm above floor level



HRRIR measurement cube IEM graz
2008-04-03 rumori

samplerate: 44100
systemlatenz: 1126.441 samples = 25.54 ms roundtrip (lt. jdelay)
sweep: 10s (21.484Hz-22kHz = 1 Oct/sec)

zwei hoehen:
- h1: 0-grad-level (ohrkanal 1370mm ueber boden)
- h2: ca. stehend-level (ohrkanal 1630 mm ueber boden,
			bzw. 1210 mm ueber boden bei dn)

mikrophone:

- b+k kunstkopf intern: kk

b+k kunstkopf
- 2 hoehen ohrkanal:
  - horizont = 1370 (mitte)
  - leichte elevation: 1630 (ueberkopf: 1110)


mit bodenbedaempfung/baffeln: