ph: panels on left half of each wall fully up, right half fully down (as shown in ASCII art below), all curtains drawn at both top and low ground level

Impulse Responses taken in the Sonic Lab Belfast (SARC)
http://www.qub.ac.uk/sites/sarc/AboutUs/TheSARCBuildingandFacilities/TheSonicLab/SonicLabSpecs/

by
Florian Hollerweger and Martin Rumori
December 2009
http://lac.linuxaudio.org/2013/papers/60.pdf


with the Neumann KU100 Dummy Head

Headphone Correction Filters applied by Matthias Kronlachner, October 2013
Headphone Correction Filters by Benjamin Bernschuetz
http://www.audiogroup.web.fh-koeln.de/ku100hrir.html